Low Current, High Voltage Power Supply

 Ahigh voltage power supply is a very useful source which can be effectively used in many applications like
 biasing of gas-discharge tubes and radiation detectors etc. Such a power supply could also be used for
 protection of property by electric charging of fences. Here the current requirement is of the order of a few
 microamps. In such an application, high voltage would essentially exist between a ‘live’ wire and ground. When
 this ‘live’ wire is touched, the discharge occurs via body resistance and it gives a non-lethal but deterrent
 shock to an intruder. The circuit is built around a single transistorised blocking oscillator. An important element
 in this circuit is the transformer. It can be fabricated on easily available ferrite cores. Two ‘E’ sections of the
 core are joined face-to-face after the enamelled copper wire wound on former is placed in it. The details of the
 transformer windings are given in the Table.

 In this configuration, the primary winding and the feedback
 winding are arranged such that a sustaining oscillation is
 ensured once the supply is switched on. The waveform’s
 duty cycle is asymmetrical, but it is not very important in this
 application. Please note that if the oscillations do not occur
 at the ‘switch-on’ time, the transformer winding terminals of
 the feedback or the primary winding (but not both) should be
 reversed. The primary oscillation amplitude is about
 24V(p-p). This gets amplified with the large step-up ratio of
 the transformer and we get about 800V(p-p) across the secondary. A simple series voltage multiplier (known
 as Cockroft-Walton circuit) is used to boost up this voltage in steps to give a final DC of about 2 kV. The output
 voltage, however, is not very well regulated. But if there is a constant load, the final voltage can be adjusted by
 varying the supply voltage. 

 The present configuration gives 2 kV for an input DC voltage of 15 V. Though higher voltages could be
 achieved by increasing input supply, one word of caution is necessary: that the component ratings have to be
 kept in mind. If the ratings are exceeded then there will be electrical discharges and breakdowns, which will
 damage the device.